**SETTINGS FOR FRING**

* **Point your mobile browser to** [**http://m.fring.com**](http://m.fring.com)
* **If you are new to fring you need to register first.**
* **After Downloading fring, Select “SIP” from Service Provider Name.**
* **Click on “Other” in SIP Service Name.**
* **A Screen will appear asking for SIP User-ID & Password.**
* **In User-ID, mention the calling pin number along with the switch ip**

**User-ID: “Your** [**Pin”@174.136.36.22**](mailto:pin@174.136.36.22)

* **In Password, mention the password of your PIN.**
* **In Proxy address, mention the IP address of the switch**

**Proxy: 174.136.36.22**

* **In order to call, Dialing pattern should be**

**Country Code + Number**